{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M2V1B","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Ventilator","Luftmængde","Køle","Super lav","m³/min","30","","","34"]
["","","Varme","Super lav","m³/min","32","","","34"]
["Lydeffekt","Opvarmning","","","dBA","","","62","","62"]
["","Køling","","","dBA","","","60","","60"]
["Ventilator","Luftmængde","Køle","Super lav","cfm","1059","","","1200"]
["","","Varme","Super lav","cfm","1130","","","1200"]
["Mål","Enhed","","Højde","mm","550","550","550","550","550","550"]
["","","","Bredde","mm","765","765","765","765","765","765"]
["","","","Dybde","mm","285","285","285","285","285","285"]
["Vægt","Enhed","","","kg","36","36","36","41","41","41"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","760","500","500","890","500","500"]
["","","Varme","Super lav","o/min","820","320","320","890","500","500"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10","","46.0","-10","46.0"]
["","","","Max.","°CDB","46","","-10","46","-10"]
["","Varme","Omgivende","Min.","°CWB","-15","","-15","-15","-15.0"]
["","","","Max.","°CWB","18","","18.0","18","18.0"]
["Lydtryk","Køle","","Høj","dBA","","46","46","","48","48"]
["","","","Nom.","dBA","48","","","46"]
["","Varme","","Høj","dBA","","48","48","","50","50"]
["","","","Nom.","dBA","50","","","48"]
["Kølemiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Belastning","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Påfyldning","","","tCO2Eq","0.6","0.59","0.6","0.8","0.78","0.78"]
["","GWP","","","","675","675.0","675","675","675","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","20","20","20 (1)","20","20 (1)","20"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 20 m)","0,02 (til rørlængde over 20 m)","0,02 (til rørlængde over 20 m)","0,02 (til rørlængde over 20 m)","0,02 (til rørlængde over 20 m)","0,02 (til rørlængde over 20 m)"]
["","Niveauforskel","IU - OU","Max.","m","15","15.0","15","15","15","15.0"]
["","","IU - IU","Max.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Samlet rørlængde","System","Nuværende","m","30","30","30","30","30","30"]
["Standardtilbehør","Installation manual","","","","Installation manual","1","1","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1","1","1"]
["Strømforsyning","Fase","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50","50","50","50"]
["","Strømspænding","","","V","220-240","220-230-240","220-230-240","220-240","220-230-240","220-230-240"]
["Bemærkninger","","","","","","(1) - Til ét rum","","","","(1) - Til ét rum"]
["","","","","","","","(1) - Til ét rum","","(1) - Til ét rum"]
["","","","","","","","(2) - Se separat tegning for driftsområde","","(2) - Se separat tegning for driftsområde"]
["","","","","","","","(3) - Se særskilte tegninger med de elektriske data","","(3) - Se særskilte tegninger med de elektriske data"]
["","","","","","","","(4) - Indeholder drivhusgasser med tilsat fluor","","(4) - Indeholder drivhusgasser med tilsat fluor"]
["Standardtilbehør","Reducer assembly","","","","","","","1","1","1"]