{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A9"]
[]
[]
[]
[]
["","","","","","2MXM40A2V1B9","2MXM50A2V1B9","2MXM68A2V1B9"]
["Mål","Enhed","","Højde","mm","552","552","734"]
["","","","Bredde","mm","852","852","974"]
["","","","Dybde","mm","350","350","408"]
["Vægt","Enhed","","","kg","36","41","60"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46"]
["Lydtryk","Køle","","Nom.","dBA","46","48","48"]
["","Varme","","Nom.","dBA","48","50","48"]
["Kølemiddel","Type","","","","R-32","R-32","R-32"]
["","Belastning","","","kg","0.88","1.15","2"]
["","Påfyldning","","","tCO2Eq","0.60","0.78","1.35"]
["","GWP","","","","675","675","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","20 (1)","20 (1)","25 (1)"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 20 m)","0,02 (til rørlængde over 20 m)","0,02 (til rørlængde over 30 m)"]
["","Niveauforskel","IU - OU","Max.","m","15","15","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Samlet rørlængde","System","Nuværende","m","30","30","50"]
["Standardtilbehør","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Energieffektivitetsklasse","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Strømforsyning","Fase","","","","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50"]
["","Strømspænding","","","V","220-240","220-240","220-240"]
["Bemærkninger","","","","","(1) - Til ét rum","(1) - Til ét rum","(1) - Til ét rum"]
["","","","","","(2) - Til kombination med CVXM-A, FVXM-A - maksimal rørlængde er 30 m.","(2) - Til kombination med CVXM-A, FVXM-A - maksimal rørlængde er 30 m.","(2) - Til kombination med CVXM-A, FVXM-A - maksimal rørlængde er 30 m."]
["","","","","","(3) - Se separat tegning for driftsområde","(3) - Se separat tegning for driftsområde","(3) - Se separat tegning for driftsområde"]
["","","","","","(4) - Se særskilte tegninger med de elektriske data","(4) - Se særskilte tegninger med de elektriske data","(4) - Se særskilte tegninger med de elektriske data"]
["","","","","","(5) - Indeholder drivhusgasser med tilsat fluor","(5) - Indeholder drivhusgasser med tilsat fluor","(5) - Indeholder drivhusgasser med tilsat fluor"]
["Standardtilbehør","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]