{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M9"]
[]
[]
[]
[]
["","","","","","2MXM50M2V1B9"]
["Mål","Enhed","","Højde","mm","550"]
["","","","Bredde","mm","765"]
["","","","Dybde","mm","285"]
["Vægt","Enhed","","","kg","41"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","500"]
["","","Varme","Super lav","o/min","500"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor"]
["Lydtryk","Køle","","Høj","dBA","48"]
["","Varme","","Høj","dBA","50"]
["Kølemiddel","Type","","","","R-32"]
["","Belastning","","","kg","1.15"]
["","Påfyldning","","","tCO2Eq","0.8"]
["","GWP","","","","675.0"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","20"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 20 m)"]
["","Niveauforskel","IU - OU","Max.","m","15.0"]
["","","IU - IU","Max.","m","7.5"]
["","Samlet rørlængde","System","Nuværende","m","30"]
["Standardtilbehør","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Strømforsyning","Fase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","220-230-240"]
["Bemærkninger","","","","","(1) - Hver eneste D-AHU Professional kan blive designet efter dine behov. Vælg din AHU på tools.daikinapplied.eu"]