{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Lydtryk","Varme","","Nom.","dBA","47"]
["","Køle","","Nom.","dBA","46"]
["Standardtilbehør","Installationsvejledning","","","","1"]
["","Skruepose","","","","1"]
["","Afløbsprop","","","","1"]
["","Afløbsdæksel (1)","","","","6"]
["","Afløbsdæksel (2)","","","","3"]
["","Tag F-gas etiketten af","","","","1"]
["","Ekstra kølemiddelmærkat","","","","1"]
["Kølemiddel","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Charge","","","kg","1.8"]
["","Type","","","","R-32"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","420"]
["","","Varme","Super lav","o/min","420"]
["Rørtilslutninger","Niveauforskel","IU - IU","Max.","m","7.5"]
["","","IU - OU","Max.","m","15"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 30 m)"]
["","Samlet rørlængde","System","Nuværende","m","50"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor"]
["Mål","Enhed","","Bredde","mm","868"]
["","","","Dybde","mm","320"]
["","","","Højde","mm","734"]
["Vægt","Enhed","","","kg","57"]
["Power supply","Fase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","220-240"]
["Bemærkninger","","","","","(1) - Indeholder drivhusgasser med tilsat fluor"]
["","","","","","(2) - Se separat tegning for driftsområde"]
["","","","","","(3) - Se særskilte tegninger med de elektriske data"]
["Ventilator","Luftmængde","Køle","Super lav","m³/min","","24"]
["","","Varme","Super lav","m³/min","","24"]
["","","","Super lav","cfm","","847"]
["","","Varme","Super lav","cfm","","847"]
["Mål","Enhed","","Højde","mm","","734"]
["","","","Bredde","mm","","868"]
["","","","Dybde","mm","","320"]
["Vægt","Enhed","","","kg","","57"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","","420"]
["","","Varme","Super lav","o/min","","420"]
["Kompressor","Type","","","","","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","","-10"]
["","","","Max.","°CDB","","46"]
["","Varme","Omgivende","Min.","°CWB","","-15"]
["","","","Max.","°CWB","","18"]
["Lydtryk","Køle","","Nom.","dBA","","46"]
["","Varme","","Nom.","dBA","","47"]
["Kølemiddel","Type","","","","","R-32"]
["","Belastning","","","kg","","1.80"]
["","Påfyldning","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","","25"]
["","Ekstra kølemiddelopladning","","","kg/m","","0,02 (til rørlængde over 30 m)"]
["","Niveauforskel","IU - OU","Max.","m","","15"]
["","","IU - IU","Max.","m","","7.5"]
["","Samlet rørlængde","System","Nuværende","m","","50"]
["Standardtilbehør","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Strømforsyning","Fase","","","","","1~"]
["","Frekvens","","","Hz","","50"]
["","Strømspænding","","","V","","220-240"]