{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-N9"]
[]
[]
[]
[]
["","","","","","3AMXM52N2V1B9"]
["Lydeffekt","Opvarmning","","","dBA","59"]
["","Køling","","","dBA","59"]
["Mål","Enhed","","Højde","mm","734"]
["","","","Bredde","mm","974"]
["","","","Dybde","mm","401"]
["Vægt","Enhed","","","kg","57"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","420"]
["","","Varme","Super lav","o/min","420"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["Lydtryk","Køle","","Nom.","dBA","46"]
["","Varme","","Nom.","dBA","47"]
["Kølemiddel","Type","","","","R-32"]
["","Belastning","","","kg","1.8"]
["","Påfyldning","","","tCO2Eq","1.22"]
["","GWP","","","","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","25 (1)"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 30 m)"]
["","Niveauforskel","IU - OU","Max.","m","15"]
["","","IU - IU","Max.","m","7.5"]
["","Samlet rørlængde","System","Nuværende","m","50"]
["Standardtilbehør","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Strømforsyning","Fase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","220-240"]
["Bemærkninger","","","","","(1) - Til ét rum"]
["","","","","","(2) - Se separat tegning for driftsområde"]
["","","","","","(3) - Se særskilte tegninger med de elektriske data"]
["","","","","","(4) - Indeholder drivhusgasser med tilsat fluor"]