{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N7"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B7","3MXM52N2V1B7","3MXM68N2V1B7"]
["Ventilator","Luftmængde","Køle","Super lav","m³/min","","","24.1"]
["","","Varme","Super lav","m³/min","","","24.1"]
["","","","Super lav","cfm","","","851"]
["","","Varme","Super lav","cfm","","","851"]
["Mål","Enhed","","Højde","mm","734","734","734"]
["","","","Bredde","mm","974","974","958"]
["","","","Dybde","mm","401","401","340"]
["Vægt","Enhed","","","kg","57","57","62"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","420","420"]
["","","Varme","Super lav","o/min","420","420"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46"]
["","Varme","Omgivende","Min.","°CWB","","","-15"]
["","","","Max.","°CWB","","","24"]
["Lydtryk","Køle","","Nom.","dBA","46","46","48"]
["","Varme","","Nom.","dBA","47","47","48"]
["Kølemiddel","Type","","","","R-32","R-32","R-32"]
["","Belastning","","","kg","1.8","1.8","2"]
["","Påfyldning","","","tCO2Eq","1.22","1.22"]
["","GWP","","","","675","675","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","25","25 (1)","25"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 30 m)","0,02 (til rørlængde over 30 m)","0,02 (til rørlængde over 30 m)"]
["","Niveauforskel","IU - OU","Max.","m","15.0","15.0","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Samlet rørlængde","System","Nuværende","m","50","50 (2)","50"]
["Standardtilbehør","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Strømforsyning","Fase","","","","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50"]
["","Strømspænding","","","V","220-240","220-240","220-440"]
["Bemærkninger","","","","","(1) - Til ét rum","(1) - Til ét rum"]
["","","","","","(2) - Til kombination med CVXM-A, FVXM-A - maksimal rørlængde er 30 m.","(2) - Til kombination med CVXM-A, FVXM-A - maksimal rørlængde er 30 m."]
["Standardtilbehør","Installationsvejledning","","","","","","1"]
["","Afløbsdæksel","","","","","","3"]
["","Afløbsprop","","","","","","1"]
["","Reduktionsmuffesamling","","","","","","1"]
["","Skruepose","","","","","","1"]
["Energieffektivitetsklasse","","","","","","","A+++ ~ D"]