{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-A8"]
[]
[]
[]
[]
["","","","","","5MXM90A2V1B8"]
["Mål","Enhed","","Højde","mm","734"]
["","","","Bredde","mm","974"]
["","","","Dybde","mm","408"]
["Vægt","Enhed","","","kg","68"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10"]
["","","","Max.","°CDB","50"]
["Lydtryk","Køle","","Nom.","dBA","52"]
["","Varme","","Nom.","dBA","52"]
["Kølemiddel","Type","","","","R-32"]
["","Belastning","","","kg","2.40"]
["","Påfyldning","","","tCO2Eq","1.62"]
["","GWP","","","","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","25 (1)"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 30 m)"]
["","Niveauforskel","IU - OU","Max.","m","15"]
["","","IU - IU","Max.","m","7.5"]
["","Samlet rørlængde","System","Nuværende","m","75"]
["Standardtilbehør","Installationsvejledning","","","","1"]
["","Afløbsdæksel","","","","3"]
["","Afløbsprop","","","","1"]
["","Reduktionsmuffesamling","","","","1"]
["","Skruepose","","","","1"]
["Energieffektivitetsklasse","","","","","A+++ ~ D"]
["Strømforsyning","Fase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","220-240"]
["Bemærkninger","","","","","(1) - Til ét rum"]
["","","","","","(2) - Til kombination med CVXM-A, FVXM-A - maksimal rørlængde er 30 m."]
["","","","","","(3) - Se separat tegning for driftsområde"]
["","","","","","(4) - Se særskilte tegninger med de elektriske data"]
["","","","","","(5) - Indeholder drivhusgasser med tilsat fluor"]