{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Kølekapacitet","Nom.","","kW","9.5","12.1 (1)"]
["Rumkøling","SEER","","","4.65","4.68"]
["","Årligt energiforbrug","","kWh/a","716","1,550"]
["","Kapacitet","Pdesign","kW","9.50","12.1"]
["","Energieffektivitetsklasse","","","B"]
["Rumopvarmning (gennemsnitsklima)","Kapacitet","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Energieffektivitetsklasse","","","A"]
["","Årligt energiforbrug","","kWh/a","2,498","3,340"]
["Nominel effektivitet","Årligt energiforbrug","","kWt","1,813"]
["","EER","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Direktiv om energimærkning","Køling","","D"]
["","","Opvarmning","","B"]
["Varmekapacitet","Nom.","","kW","10.8","13.5 (2)"]
["Bemærkninger","","","","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB; tilsvarende rørlængde: 7,5 m, niveauforskel: 0m"]
["","","","","(2) - Årligt energiforbrug ifølge Direktivet for energimærkning 2002/31/EC","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 7,5 m, niveauforskel: 0m"]
["","","","","(3) - SEER og SCOP er i overensstemmelse med EN 14825","(3) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU"]
["","","","","(4) - Nominel effektivitet: Køling ved 35°/27° nominel belastning, opvarmning ved 7°/20° nominel belastning"]