{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEA100A2VEB / AZQS100B8V1B","ADEA125A2VEB / AZQS125B8V1B"]
["Kølekapacitet","Nom.","","kW","9.50","12.10"]
["Rumkøling","SEER","","","5.10","4.83"]
["","Årligt energiforbrug","","kWh/å","652","1,504"]
["","Kapacitet","Pdesign","kW","9.50","12.10"]
["","Energieffektivitetsklasse","","","A"]
["Rumopvarmning (gennemsnitsklima)","Kapacitet","Pdesign","kW","7.60","7.93"]
["","SCOP/A","","","3.81","3.50"]
["","Energieffektivitetsklasse","","","A"]
["","Årligt energiforbrug","","kWh/å","2,793","3,167"]
["Nominel effektivitet","EER","","","","2.27"]
["Varmekapacitet","Nom.","","kW","10.80","13.50"]
["Bemærkninger","","","","(1) - Se separat tegning for driftsområde","(1) - Se separat tegning for driftsområde"]
["","","","","(2) - Se særskilte tegninger med de elektriske data","(2) - Se særskilte tegninger med de elektriske data"]
["","","","","(3) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB; tilsvarende rørlængde: 7,5 m, niveauforskel: 0m","(3) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB; tilsvarende rørlængde: 7,5 m, niveauforskel: 0m"]
["","","","","(4) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 7,5 m, niveauforskel: 0m","(4) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 7,5 m, niveauforskel: 0m"]