{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Indgangseffekt","Varme","","Nom.","kW","0.106","0.149"]
["","Køle","","Nom.","kW","0.106","0.149"]
["Ventilator","Udvendigt statisk tryk","","Høj","Pa","0","0","0","0"]
["","","","Lav","Pa","0","0","0","0"]
["Kølekapacitet","Samlet kapacitet","","Nom.","kW","","","12.10","13.00"]
["Varmekapacitet","Samlet kapacitet","","Nom.","kW","","","13.5","15.5"]
["Kabinet","Farve","","","","Hvid","Hvid","Hvid","Hvid"]
["","Materiale","","","","Galvaniseret stål","Galvaniseret stål"]
["Mål","Enhed","","Højde","mm","260","260","260","285"]
["","","","Bredde","mm","1320","1538","1790","1900"]
["","","","Dybde","mm","634","634","634","680"]
["Vægt","Enhed","","","kg","38","45","65","70"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","31","39"]
["","","Køling","Mellem","m³/min","","","31","39"]
["","","","Lav","m³/min","18.9","24.8","27.2","28.3"]
["","","Varme","Høj","m³/min","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min","21.3","27.8","30.6","39.1"]
["","","Opvarmning","Mellem","m³/min","","","30.6","39.1"]
["","","Varme","Lav","m³/min","18.9","24.8","27.2","28.3"]
["","Udvendigt statisk tryk","","Nom.","Pa","0","0","0","0"]
["Lydeffekt","Køling","","","dBA","59","64","65","71"]
["","Opvarmning","","","dBA","62","64","65","71"]
["Lydtryk","Køle","","Høj","dBA","49","52","52","56"]
["","","","Nom.","dBA","48","47"]
["Lydtryksniveau","Køling","","Mellem","dBA","","","50","53"]
["Lydtryk","Køle","","Lav","dBA","46","46","49","46"]
["","Varme","","Høj","dBA","49","52","52","56"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","","","50","53"]
["Lydtryk","Varme","","Nom.","dBA","48","47"]
["","","","Lav","dBA","46","46","49","46"]
["Rørtilslutninger","Flydende","","UD","mm","9.52","9.52","9.52","9.52"]
["","Gas","","UD","mm","15.88","15.88","15.9","15.9"]
["","Dræn","","","","19.05","19.05"]
["Styresystemer","Trådløs fjernbetjening","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Fortrådet fjernbetjening","","","","ARCWB","ARCWB"]
["Standardtilbehør","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Afløbsrør","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Strømforsyning","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","220-240","220-240"]