{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Lydtryk","Varme","","Nom.","dBA","","49.0"]
["","Køle","","Nom.","dBA","","49.0"]
["Standardtilbehør","Afløbsprop","","","","","1"]
["","Installationsvejledning","","","","","1"]
["","Mærkat for kølemiddelmængde","","","","","1"]
["","Flersproget mærkat for fluorholdige drivhusgasser","","","","","1"]
["","Generelle sikkerhedsforholdsregler","","","","","1"]
["Kølemiddel","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Belastning","","","kg","","0.76"]
["","Type","","","","","R-32"]
["Driftsområde","Køle","Omgivende","Max.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Piping connections","Niveauforskel","IU - OU","Max.","m","","15"]
["","Ekstra kølemiddelopladning","","","kg/m","","0,02 (til rørlængde over 10 m)"]
["Kompressor","Type","","","","","Hermetisk lukket svingkompressor"]
["Mål","Enhed","","Bredde","mm","","840"]
["","","","Dybde","mm","","350"]
["","","","Højde","mm","","552"]
["Vægt","Enhed","","","kg","","32"]
["Power supply","Phase","","","","","1~"]
["","Frekvens","","","Hz","","50"]
["","Strømspænding","","","V","","220-240"]
["Bemærkninger","","","","","(1) - Kun muligt i kombination med ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Indeholder drivhusgasser med tilsat fluor"]
["","","","","","(2) - Kun muligt i kombination med ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Se separat tegning for driftsområde"]
["","","","","","","(3) - Se særskilte tegninger med de elektriske data"]
["","","","","","","(4) - Kun muligt i kombination med ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Kun muligt i kombination med ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Mål","Enhed","","Højde","mm","552"]
["","","","Bredde","mm","840"]
["","","","Dybde","mm","350"]
["Vægt","Enhed","","","kg","32"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10"]
["","","","Max.","°CDB","50 (4), 46 (5)"]
["Lydtryk","Køle","","Nom.","dBA","46.0"]
["","Varme","","Nom.","dBA","47.0"]
["Kølemiddel","Belastning","","","kg","0.76"]
["","Påfyldning","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","20"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 10 m)"]
["","Niveauforskel","IU - OU","Max.","m","15"]
["Standardtilbehør","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Strømforsyning","Frekvens","","","Hz","50"]