{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Lydtryk","Varme","","Høj","dBA","","","47","48"]
["","","","Nom.","dBA","","52","","","49"]
["","Køle","","Høj","dBA","","","46","48"]
["","","","Nom.","dBA","","52","","","49"]
["Standardtilbehør","Afløbsprop","","","","","1","1","1","1"]
["","Installationsvejledning","","","","","1","1","1","1"]
["","Mærkat for kølemiddelmængde","","","","","1","1","","1"]
["","Flersproget mærkat for fluorholdige drivhusgasser","","","","","1","1","","1"]
["Kølemiddel","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Opladning","","","kg","","1.70","1.0","1.2","1.50"]
["","Type","","","","","R-410A","R-410A","R-410A","R-410A"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","","","780","780"]
["","","Varme","Super lav","o/min","","","740","740"]
["Driftsområde","Køling","Omgivende","Max.","°CDB","","46","46","46","46"]
["","","","Min.","°CDB","","-10","10","10","-10"]
["","Opvarmning","Omgivende","Max.","°CWB","","18","18","18","18"]
["","","","Min.","°CWB","","-15","-15","-15","-15"]
["Piping connections","Niveauforskel","IU - OU","Max.","m","","20.0","15","15","20.0"]
["","Ekstra kølemiddelopladning","","","kg/m","","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)"]
["Sound power level","Køling","","","dBA","","65","","","62"]
["","Opvarmning","","","dBA","","65","","","62"]
["Kompressor","Type","","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Dimensioner","Enhed","","Bredde","mm","","825","765","765","825"]
["","","","Dybde","mm","","300","285","285","300"]
["","","","Højde","mm","","735","550","550","735"]
["Vægt","Enhed","","","kg","","47","34","34","47"]
["Ventilator","Luftmængde","Varme","Super lav","cfm","","","904","904"]
["","","","Super lav","m³/min","","","25.6","25.6"]
["","","Køle","Super lav","m³/min","","","30.1","30.1"]
["","","","Super lav","cfm","","","1,063","1,063"]
["Power supply","Fase","","","","","1~","1~","1~","1~"]
["","Frekvens","","","Hz","","50","50","50","50"]
["","Strømspænding","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Bemærkninger","","","","","(1) - 220V","","(1) - Læs specifikationer til den Multi udendørs enhed, der skal tilsluttes, når den er koblet til udendørs enhed i Multi-system.","(1) - Læs specifikationer til den Multi udendørs enhed, der skal tilsluttes, når den er koblet til udendørs enhed i Multi-system."]
["","","","","","(2) - 230V","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","","(3) - 230V","(3) - 230V"]
["","","","","","","","(4) - 240V","(4) - 240V"]
["","","","","","","","(5) - Indeholder drivhusgasser med tilsat fluor","(5) - Indeholder drivhusgasser med tilsat fluor"]
["Ventilator","Luftmængde","Køle","Super lav","m³/min","48.9"]
["","","Varme","Super lav","m³/min","43.1"]
["","","","Super lav","cfm","1727"]
["","","Varme","Super lav","cfm","1522"]
["Mål","Enhed","","Højde","mm","735"]
["","","","Bredde","mm","825"]
["","","","Dybde","mm","300"]
["Vægt","Enhed","","","kg","47"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","670"]
["","","Varme","Super lav","o/min","670"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","10"]
["","","","Max.","°CDB","46"]
["","Varme","Omgivende","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Lydtryk","Køle","","Høj","dBA","48"]
["","Varme","","Høj","dBA","48"]
["Kølemiddel","Type","","","","R-410A"]
["","Belastning","","","kg","1.7"]
["","Påfyldning","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","30"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 10 m)"]
["","Niveauforskel","IU - OU","Max.","m","20"]
["Standardtilbehør","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Strømforsyning","Fase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","220-240"]
["Bemærkninger","","","","","","(1) - Indeholder drivhusgasser med tilsat fluor","","","(1) - Indeholder drivhusgasser med tilsat fluor"]