{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Lydtryk","Varme","","Høj","dBA","","48"]
["","","","Lav","dBA","","45"]
["Standardtilbehør","1","","","","","550"]
["Kølemiddel","Belastning","","","kg","","2.5"]
["","Type","","","","","1.2"]
["Ventilator","Luftmængde","Køling","Super lav","m³/min","","30.1"]
["","","","Super lav","cfm","","1,063"]
["Blæsermotor","Hastighed","Køle","Super lav","o/min","","740"]
["","","Varme","Super lav","o/min","","-15"]
["Driftsområde","Heating","Omgivende","Min.","°CWB","","20"]
["","","","Max.","°CWB","","10"]
["Lydtryk","Køle","","Lav","dBA","","44"]
["","","","Høj","dBA","","48"]
["Kompressor","Type","","","","","Hermetisk lukket svingkompressor"]
["Mål","Enhed","","Bredde","mm","","285"]
["","","","Dybde","mm","","612"]
["","","","Højde","mm","","765"]
["Vægt","Enhed","","","kg","","34"]
["Ventilator","Luftmængde","Varme","Super lav","cfm","","904"]
["","","","Super lav","m³/min","","25.6"]
["Power supply","Phase","","","","","1~"]
["","Frekvens","","","Hz","","50"]
["","Strømspænding","","","V","","220-240"]
["Bemærkninger","","","","","(1) - 220V","(1) - Indeholder drivhusgasser med tilsat fluor"]
["","","","","","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 230V"]
["","","","","","","(4) - 240V"]
["Ventilator","Luftmængde","Køle","Super lav","m³/min","30.1"]
["","","Varme","Super lav","m³/min","25.6"]
["","","","Super lav","cfm","1063"]
["","","Varme","Super lav","cfm","904"]
["Mål","Enhed","","Højde","mm","550"]
["","","","Bredde","mm","765"]
["","","","Dybde","mm","285"]
["Vægt","Enhed","","","kg","34"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","780"]
["","","Varme","Super lav","o/min","740"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","10"]
["","","","Max.","°CDB","46"]
["","Varme","Omgivende","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Lydtryk","Køle","","Høj","dBA","46"]
["","Varme","","Høj","dBA","47"]
["","","","Lav","dBA","44"]
["Kølemiddel","Type","","","","R-410A"]
["","Belastning","","","kg","1.0"]
["","Påfyldning","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","20"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 10 m)"]
["","Niveauforskel","IU - OU","Max.","m","15"]
["Standardtilbehør","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Strømforsyning","Fase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","220-240"]