{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Lydtryk","Varme","","Høj","dBA","","","","","","43"]
["","","","Mellem","dBA","","","","","","35"]
["","","","Lydsvag drift","dBA","","","","","","26"]
["","","","Lav","dBA","","","","","","29"]
["","Køle","","Mellem","dBA","","","","","","34"]
["","","","Lydsvag drift","dBA","","","","","","20"]
["","","","Lav","dBA","","","","","","27"]
["","","","Høj","dBA","","","","","","43"]
["Standardtilbehør","Installationsvejledning","","","","","","","","","1"]
["","Betjeningsvejledning","","","","","","","","","1"]
["","Trådløs fjernbetjening","","","","","","","","","1"]
["","AA tørcelle batteriet","","","","","","","","","2"]
["","Holder til fjernbetjening","","","","","","","","","1"]
["","Monteringsplade","","","","","","","","","1"]
["","Fotokatalytisk luftrenserfilter med titaniumapatit","","","","","","","","","2"]
["","Fastgøringsskruer til indendørs enhed","","","","","","","","","2"]
["Styresystemer","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Rørtilslutninger","Flydende","","UD","mm","","","","","","6.35"]
["","Gas","","UD","mm","","","","","","9.50"]
["","Dræn","","","","","","","","","18"]
["Strømforbrug","Køle","","Nom.","kW","","","","","","0.024"]
["","Varme","","Nom.","kW","","","","","","0.029"]
["Sound power level","Køling","","","dBA","","","","","","58"]
["","Opvarmning","","","dBA","","","","","","58"]
["Mål","Enhed","","Bredde","mm","","","","","","770"]
["","","","Dybde","mm","","","","","","225"]
["","","","Højde","mm","","","","","","286"]
["Kabinet","Farve","","","","","","","","","Hvid"]
["Vægt","Enhed","","","kg","","","","","","9.0"]
["Power supply","Fase","","","","","","","","","1~"]
["","Frekvens","","","Hz","","","","","","50"]
["","Navn","","","","","","","","","V1"]
["","Strømspænding","","","V","","","","","","220-240"]
["Bemærkninger","","","","","","","","","","(1) - SL: Luftstrømmens hastighedsindstillings lydløse ventilatorniveau"]
["Indgangseffekt","Køle","","Nom.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Varme","","Nom.","kW","0.022","0.022","0.023","0.023","0.029"]
["Kabinet","Farve","","","","Hvid","Hvid","Hvid","Hvid","Hvid"]
["Mål","Enhed","","Højde","mm","286","286","286","286","286"]
["","","","Bredde","mm","770","770","770","770","770"]
["","","","Dybde","mm","225","225","225","225","225"]
["Vægt","Enhed","","","kg","8.5","8.5","8.5","8.5","9"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","","Køling","Mellem","m³/min","7.8","7.8","8","8","8.2"]
["","","","Lav","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Lydsvag drift","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Varme","Høj","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","","Opvarmning","Mellem","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","Varme","Lav","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Lydsvag drift","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Lydeffekt","Køling","","","dBA","55","55","55","55","58"]
["","Opvarmning","","","dBA","55","55","55","55","58"]
["Lydtryk","Køle","","Høj","dBA","39","39","40","40","43"]
["Lydtryksniveau","Køling","","Mellem","dBA","33","33","33","33","34"]
["Lydtryk","Køle","","Lav","dBA","25","25","26","26","27"]
["","","","Lydsvag drift","dBA","20","20","20","20","20"]
["","Varme","","Høj","dBA","39","39","40","40","43"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","34","34","34","34","35"]
["Lydtryk","Varme","","Lav","dBA","28","28","28","28","29"]
["","","","Lydsvag drift","dBA","23","23","23","23","26"]
["Rørtilslutninger","Flydende","","UD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","UD","mm","9.5","9.5","9.5","9.5","9.5"]
["","Dræn","","","","18","18","18","18","18"]
["Styresystemer","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Styresystemer","Fortrådet fjernbetjening","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardtilbehør","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Strømforsyning","Navn","","","","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50","50","50"]
["","Strømspænding","","","V","220-240","220-240","220-240","220-240","220-240"]
["Standardtilbehør","AAA dry-cell batteries","","","","","2","","2","2"]
["Styresystemer","Trådløs fjernbetjening","","","","","","ARC480A11","ARC480A11"]
["Standardtilbehør","Titanium apatite photocatalytic air purification filter","","","","","","2"]