{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-D"]
[]
[]
[]
[]
["","","","","","ATXF20D5V1B","ATXF25D5V1B","ATXF35D5V1B","ATXF42D5V1B"]
["Indgangseffekt","Køle","","Nom.","kW","0.023","0.023","0.029","0.040"]
["","Varme","","Nom.","kW","0.023","0.023","0.029","0.040"]
["Kabinet","Farve","","","","Hvid","Hvid","Hvid","Hvid"]
["Mål","Enhed","","Højde","mm","286","286","286","286"]
["","","","Bredde","mm","770","770","770","770"]
["","","","Dybde","mm","225","225","225","225"]
["Vægt","Enhed","","","kg","8","8","8.5","9.00"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","9.8","10","11.5","12.6"]
["","","Køling","Mellem","m³/min","8","8","8","9"]
["","","","Lav","m³/min","6","6.2","6.4","6.9"]
["","","","Lydsvag drift","m³/min","4.3","4.3","4.4","4.9"]
["","","Varme","Høj","m³/min","10.4","10.4","11.9","12.8"]
["","","Opvarmning","Mellem","m³/min","8.3","8.4","8.6","8.8"]
["","","Varme","Lav","m³/min","6.2","6.4","6.5","6.7"]
["","","","Lydsvag drift","m³/min","5.3","5.3","5.3","5.2"]
["Lydeffekt","Køling","","","dBA","53","54","54","59.0"]
["","Opvarmning","","","dBA","55","55","56","59.0"]
["Lydtryk","Køle","","Høj","dBA","39","40","43","45.0"]
["Lydtryksniveau","Køling","","Mellem","dBA","33","33","34","36.0"]
["Lydtryk","Køle","","Lav","dBA","25","26","27","30.0"]
["","","","Lydsvag drift","dBA","20","20","20","22.0"]
["","Varme","","Høj","dBA","39","40","40","44.0"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","34","34","35","34.0"]
["Lydtryk","Varme","","Lav","dBA","28","28","29","28.0"]
["","","","Lydsvag drift","dBA","21","21","21","22.0"]
["Rørtilslutninger","Flydende","","UD","mm","6","6","6","6"]
["","Gas","","UD","mm","9.5","9.5","9.5","9.50"]
["","Dræn","","","","18","18","18","18"]
["Styresystemer","Trådløs fjernbetjening","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["","Fortrådet fjernbetjening","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardtilbehør","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Operation manual","","","","1","1","1","1"]
["","Batteries","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Strømforsyning","Fase","","","","1~","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50","50"]
["","Strømspænding","","","V","220-440","220-440","220-440","220-440"]