{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F / ARXF-A9"]
[]
[]
[]
[]
["","","","","ATXF60F2V1B / ARXF60A5V1B9","ATXF71F2V1B / ARXF71A5V1B9"]
["Kølekapacitet","Min.","","kW","1.7","2.3"]
["","Nom.","","kW","6","7.1"]
["","Max.","","kW","7","7.3"]
["Varmekapacitet","Min.","","kW","1.7","2.3"]
["","Nom.","","kW","6.4","8.2"]
["","Max.","","kW","8","9"]
["Nominel effektivitet","EER","","","3.25","2.53"]
["","COP","","","3.9","3.12"]
["","Årligt energiforbrug","","kWh","923","1,403"]
["","Direktiv om energimærkning","Køling","","A","E"]
["","","Opvarmning","","A","D"]
["Rumkøling","Energieffektivitetsklasse","","","A++","A"]
["","Kapacitet","Pdesign","kW","6","7.1"]
["","SEER","","","6.12","5.12"]
["","Årligt energiforbrug","","kWh/a","343","486"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A+","A"]
["","Kapacitet","Pdesign","kW","4.8","6.2"]
["","SCOP/A","","","4.03","3.81"]
["","Pdh varmekapacitet ved -10°","","kW","4.24","5.02"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/a","1,668","2,278"]