{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F"]
[]
[]
[]
[]
["","","","","","ATXF50F5V1B"]
["Indgangseffekt","Køle","","Nom.","kW","0.04"]
["","Varme","","Nom.","kW","0.04"]
["Kabinet","Farve","","","","Hvid"]
["Mål","Enhed","","Højde","mm","286"]
["","","","Bredde","mm","770"]
["","","","Dybde","mm","225"]
["Vægt","Enhed","","","kg","9"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","12.6"]
["","","Køling","Mellem","m³/min","9"]
["","","","Lav","m³/min","7.2"]
["","","","Lydsvag drift","m³/min","6.4"]
["","","Varme","Høj","m³/min","12.8"]
["","","Opvarmning","Mellem","m³/min","9.6"]
["","","Varme","Lav","m³/min","7.2"]
["","","","Lydsvag drift","m³/min","6.4"]
["Lydeffekt","Køling","","","dBA","59"]
["","Opvarmning","","","dBA","59"]
["Lydtryk","Køle","","Høj","dBA","45"]
["Lydtryksniveau","Køling","","Mellem","dBA","39"]
["Lydtryk","Køle","","Lav","dBA","34"]
["","","","Lydsvag drift","dBA","31"]
["","Varme","","Høj","dBA","44"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","38"]
["Lydtryk","Varme","","Lav","dBA","33"]
["","","","Lydsvag drift","dBA","30"]
["Rørtilslutninger","Flydende","","UD","mm","6"]
["","Gas","","UD","mm","12.7"]
["","Dræn","","","","18"]
["Styresystemer","Trådløs fjernbetjening","","","","ARC480A93"]
["","Fortrådet fjernbetjening","","","","BRC073A1"]
["Standardtilbehør","ATXF50F5V1B","","","","1"]
["","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Strømforsyning","Fase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","220-440"]
["Bemærkninger","","","","","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB; tilsvarende rørlængde: 5m, niveauforskel: 0m"]
["","","","","","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5 m (vandret)"]
["","","","","","(3) - Se særskilte tegninger med de elektriske data"]