{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":9,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-M"]
[]
[]
[]
[]
["","","","","","ATXM20M2V1B (Archived)","ATXM25M2V1B (Archived)","ATXM35M2V1B (Archived)","ATXM50M2V1B (Archived)"]
["Indgangseffekt","Køle","","Nom.","kW","0.03","0.03","0.035","0.03"]
["","Varme","","Nom.","kW","0.025","0.025","0.025","0.032"]
["Kabinet","Farve","","","","Hvid","Hvid","Hvid","Hvid"]
["Mål","Enhed","","Højde","mm","294","294","294","300"]
["","","","Bredde","mm","811","811","811","1040"]
["","","","Dybde","mm","272","272","272","295"]
["Vægt","Enhed","","","kg","10","10","10","14.5"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","11.1","11.1","12.6","16.5"]
["","","Køling","Mellem","m³/min","7.9","8.1","8.3","14.2"]
["","","","Lav","m³/min","6","6.2","6.4","11.6"]
["","","","Lydsvag drift","m³/min","4.4","4.4","4.6","10.3"]
["","","Varme","Høj","m³/min","10.4","10.4","10.4","17.1"]
["","","Opvarmning","Mellem","m³/min","8.7","8.7","9","14.6"]
["","","Varme","Lav","m³/min","6.5","6.8","7.1","12.2"]
["","","","Lydsvag drift","m³/min","5.3","5.3","5.3","10.7"]
["Lydeffekt","Køling","","","dBA","58","58","60","59"]
["","Opvarmning","","","dBA","55","55","55","58"]
["Lydtryk","Køle","","Høj","dBA","41","41","45","44"]
["Lydtryksniveau","Køling","","Mellem","dBA","33","33","33","40"]
["Lydtryk","Køle","","Lav","dBA","25","25","29","36"]
["","","","Lydsvag drift","dBA","19","19","19","32"]
["","Varme","","Høj","dBA","39","39","39","43"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","34","34","35","39"]
["Lydtryk","Varme","","Lav","dBA","26","27","28","34"]
["","","","Lydsvag drift","dBA","20","20","20","31"]
["Rørtilslutninger","Flydende","","UD","mm","6.35","6.35","6.35","6.35"]
["","Gas","","UD","mm","9.5","9.5","9.5","12.7"]
["","Dræn","","","","18","18","18","18"]
["Styresystemer","Trådløs fjernbetjening","","","","ARC466A33","ARC466A33","ARC466A33","ARC466A33"]
["Styresystemer","Fortrådet fjernbetjening","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073"]
["Standardtilbehør","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","2"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Strømforsyning","Navn","","","","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50","50"]
["","Strømspænding","","","V","220-240","220-240","220-240","220-240"]