{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MY1"]
[]
[]
[]
[]
["","","","","","AZAS100M7Y1B","AZAS125M7Y1B","AZAS140M7Y1B"]
["Mål","Enhed","","Højde","mm","990","990","990"]
["","","","Bredde","mm","940","940","940"]
["","","","Dybde","mm","320","320","320"]
["Vægt","Unit","","","kg","","70"]
["Kompressor","Type","","","","","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-5","-5","-5"]
["","","","Max.","°CDB","46","46","46"]
["","Varme","Omgivende","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","15.5","15.5","15.5"]
["Lydeffekt","Køling","","","dBA","70","71","73"]
["","Opvarmning","","","dBA","","71","73 (1)"]
["Lydtryk","Køle","","Nom.","dBA","53","53","54"]
["","Varme","","Nom.","dBA","57","57","57"]
["Kølemiddel","Type","","","","R-32","R-32","R-32"]
["","Kølemiddel-=-Opladning-=-kg","","","kg","","2.60"]
["Kølemiddel","GWP","","","","","675"]
["Kølemiddel","Påfyldning","","","tCO2Eq","1.76","1.76","1.96"]
["Rørtilslutninger","Flydende","","UD","mm","9.52","9.52","9.52"]
["Rørføringsforbindelser","Gas","","UD","mm","","15.9"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","30","30","30"]
["","","System","Tilsvarende – ELLER – Lig med","m","50","50","50"]
["","","","Opladningsfri","m","30","30","30"]
["","Ekstra kølemiddelopladning","","","kg/m","Læs installationsvejledningen","Læs installationsvejledningen","Læs installationsvejledningen"]
["","Niveauforskel","IU - OU","Max.","m","30.0","30.0","30.0"]
["","","IU - IU","Max.","m","0.5","0.5","0.5"]
["Standardtilbehør","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Strømforsyning","Fase","","","","3~","3~","3~"]
["","Strømforsyning-=-Frekvens","","Frekvens","","50","50","50"]
["","Strømforsyning-=-Strømspænding","","Strømspænding","","380-415","380-415","380-415"]
["Effekt - 50 Hz","Effekt - 50 Hz-=-Max. ampere i sikring (MFA)","","Effekt - 50 Hz-=-Max. ampere i sikring (MFA)-=-A","","","16"]
["Bemærkninger","","","","","","(1) - I henhold til ENER Lot 21","(1) - I henhold til ENER Lot 21"]
["Vægt","Enhed","","","kg","70","","77"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","","Hermetisk lukket svingkompressor"]
["Kølemiddel","Belastning","","","kg","2.60","","2.90"]
["","GWP","","","","675","","675"]
["Rørtilslutninger","Gas","","UD","mm","15.9","","15.9"]
["Strøm - 50 Hz","Maksimal sikring amp (MFA)","","","A","16","","16"]