{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDW"]
[]
[]
[]
[]
["","","","","BRC1HHDAW"]
["Kabinet","Farve","","","Hvid"]
["","Knapdæksel","","","Nej"]
["","Drifts LED","Farve","","Blå statusindikator"]
["Mål","Enhed","Højde","mm","85"]
["","","Bredde","mm","85"]
["","","Dybde","mm","25"]
["","Pakket enhed","Højde","mm","50"]
["","","Bredde","mm","217"]
["","","Dybde","mm","161"]
["Vægt","Enhed","","kg","0.110"]
["","Pakket enhed","","kg","0.317"]
["Pakke","Materiale","","","Pap"]
["","Vægt","","kg","0.0850"]
["LCD","Type","","","100 x 150 dot"]
["","Dimensioner","Højde","mm","40.7"]
["","","Bredde","mm","28.0"]
["","Baggrundsbelysning","Farve","","Hvid"]
["Omgivende temperatur","Drift","Min.","°C","-10"]
["","","Max.","°C","52"]
["","Lagring","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Omgivende temperatur-=-Relativ luftfugtighed <-=-%","","%","95"]
["Styresystemer","Klasse for temperaturstyring","","","VI"]
["","Bidrag til helårs virkningsgrad for rumopvarmning","","%","4.0"]
["Kabelforbindelser","Kabellængde","Max.","m","500"]