{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32 / 3MXM-N"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32 / 3MXM52N2V1B","CHYHBH05AAV32 / 3MXM68N2V1B","CHYHBH05AFV32 / 3MXM52N2V1B","CHYHBH05AFV32 / 3MXM68N2V1B"]
["Varmtvandsvarmer","Generelt","","Erklæret belastningsprofil","","XL","XL"]
["","Gennemsnitsklima","","Energieffektivitetsklasse for vandopvarmning","","A","A"]
["COP","","","","","4.49 (1)","3.91 (1)","4.49","3.91"]
["Rumopvarmning","Vandudgang på 55 °C ved gennemsnitsklima","Generelt","Seasonal space heating eff. class","","A+","A+"]
["","","","ηs (Effektivitet for rumopvarmning på helårsbasis)","%","111.4","113.3"]
["","","","SCOP","","2.86","2.91"]
["Varmekapacitet","Nom.","","","kW","4.41 (1)","4.50 (1)"]
["Bemærkninger","","","","","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), kedel omledt","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), kedel omledt","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), kedel omledt","(1) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), kedel omledt"]
["Varmekapacitet","Nom.","","","kW","","","4.41","4.5"]
["Opvarmning af varmt brugsvand","Generelt","","Erklæret belastningsprofil","","","","XL","XL"]
["","Gennemsnitsklima","","Energieffektivitetsklasse for vandopvarmning","","","","A","A"]
["Rumopvarmning","Vandudgang på 55 °C ved gennemsnitsklima","Generelt","SCOP","","","","2.86","2.91"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","","","A+","A+"]