{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CKHWSU-BV3"]
[]
[]
[]
[]
["","","","","","CKHWSU230BJV3"]
["Dimensioner","Enhed","Højde","Tank","mm","1855"]
["Mål","Enhed","","Bredde","mm","595"]
["","","","Dybde","mm","634"]
["Vægt","Enhed","","Tom","kg","115"]
["Tank","Vandmængde","","","l","230"]
["","Materiale","","","","Rustfrit stål (DIN 1.4521)"]
["","Maksimal vandtemperatur","","","°C","65.0"]
["","Klasse for energieffektivitet","","","","C"]
["Reservevarmer","Kapacitet","","","kW","1.5"]
["Bemærkninger","","","","","(1) - Baseret på dT på 45 K"]
["","","","","","(2) - Flow for varmt brugsvand"]
["","","","","","(3) - 2-polet 10 A, kurve 230 V"]
["","","","","","(4) - Ovennævnte strømforsyning til hydroboksen er kun til sikkerhedsvarmeren. Kontaktboksen og pumpe for hydroboks forsynes via den udendørs enhed."]