{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AW"]
[]
[]
[]
[]
["","","","","","CTXA15A2V1BW"]
["Lydtryk","Varme","","Høj","dBA","39"]
["","","","Mellem","dBA","32"]
["","","","Lydsvag drift","dBA","21"]
["","","","Lav","dBA","25"]
["","Køle","","Mellem","dBA","32"]
["","","","Lydsvag drift","dBA","21"]
["","","","Lav","dBA","25"]
["","","","Høj","dBA","39"]
["Standardtilbehør","Installationsvejledning","","","","1"]
["","Betjeningsvejledning","","","","1"]
["","Luftfilter","","","","2"]
["","Trådløs fjernbetjening","","","","1"]
["","Fjernbetjeningens monteringsplade","","","","1"]
["","Skruepose","","","","1"]
["","Skruedæksel","","","","1"]
["","AAA tørcelle batteriet","","","","2"]
["","Generelle sikkerhedsforholdsregler","","","","1"]
["Kølemiddel","GWP","","","","675.0"]
["Styresystemer","Fortrådet fjernbetjening","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Rørtilslutninger","Flydende","","UD","mm","6.35"]
["","Gas","","UD","mm","9.50"]
["","Dræn","","","","18"]
["Indgangseffekt","Køle","","Nom.","kW","0.020"]
["","Varme","","Nom.","kW","0.020"]
["Lydeffekt","Køling","","","dBA","57"]
["Mål","Enhed","","Bredde","mm","798"]
["","","","Dybde","mm","189"]
["","","","Højde","mm","295"]
["Kabinet","Farve","","","","Hvid"]
["Vægt","Enhed","","","kg","12"]
["Blæser","Luftmængde","Varme","Høj","m³/min","10.9"]
["","","","Mellem","m³/min","8.7"]
["","","","Lav","m³/min","6.4"]
["","","","Lydsvag drift","m³/min","4.5"]
["","","Køle","Lav","m³/min","6.1"]
["","","","Mellem","m³/min","8"]
["","","","Høj","m³/min","11.0"]
["","","","Lydsvag drift","m³/min","4.6"]
["Power supply","Fase","","","","1~"]
["","Navn","","","","V1"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","220-240"]