{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M / 3MXM-M"]
[]
[]
[]
[]
["","","","","CTXM15M2V1B / CTXM15M2V1B / 3MXM40M2V1B","CTXM15M2V1B / CTXM15M2V1B / CTXM15M2V1B / 3MXM40M2V1B"]
["Kølekapacitet","Nom.","","kW","3.00","4.00"]
["Nominel effektivitet","Årligt energiforbrug","","kWt","293","386"]
["","EER","","","5.12","5.18"]
["","COP","","","5.25","5.32"]
["","Direktiv om energimærkning","Køling","","A","A"]
["","","Opvarmning","","A","A"]
["Varmekapacitet","Nom.","","kW","3.60","4.60"]
["Bemærkninger","","","","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU"]
["","","","","(2) - Nominel effektivitet: Køling ved 35°/27° nominel belastning, opvarmning ved 7°/20° nominel belastning","(2) - Nominel effektivitet: Køling ved 35°/27° nominel belastning, opvarmning ved 7°/20° nominel belastning"]