{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":11,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVZ-D6V / EPGA011-016DV"]
[]
[]
[]
[]
["","","","","","EAVZ16S23DA6V / EPGA11DAV3","EAVZ16S18DA6V / EPGA11DAV3","EAVZ16S18DA6V / EPGA14DAV3","EAVZ16S23DA6V / EPGA14DAV3","EAVZ16S18DA6V / EPGA16DAV3","EAVZ16S23DA6V / EPGA16DAV3"]
["Opvarmning af varmt brugsvand","Generelt","","Erklæret belastningsprofil","","XL","","L","XL","L","XL"]
["","Gennemsnitsklima","","Energieffektivitetsklasse for vandopvarmning","","A","","A","A","A","A"]
["COP","","","","","5.15 (1), 3.88 (2)","5.15, 3.88","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Indendørs enhed","","","","","EAVZ16S23DA6V","EAVZ16S18DA6V","EAVZ16S18DA6V","EAVZ16S23DA6V","EAVZ16S18DA6V","EAVZ16S23DA6V"]
["Varmekapacitet","Nom.","","","kW","11.1 (1), 11.3 (2)","","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)"]
["Strømforbrug","Varme","","Nom.","kW","2.16 (1), 2.91 (2)","","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)"]
["Bemærkninger","","","","","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]
["Varmekapacitet","Nom.","","","kW","","11.1, 11.3"]
["Indgangseffekt","Varme","","Nom.","kW","","2.16, 2.91"]
["Strømforbrug","Opvarmning af brugsvand fra 10°C til 50 °C","","Nom.","kWh","","2.67"]
["Opvarmningstid fra 10°C til 50 °C","tim","","","","","9t20min ved 7 °C omgivende temperatur"]
["Opvarmning af varmt brugsvand","Generelt","","Erklæret belastningsprofil","","","L"]
["","Gennemsnitsklima","","Energieffektivitetsklasse for vandopvarmning","","","A"]
["Rumopvarmning","Vandudgang på 55 °C ved gennemsnitsklima","Generelt","SCOP","","","3.29"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","","A++"]
["","Vandudgang på 35°C ved gennemsnitsklima","Generelt","SCOP","","","4.38"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","","A++"]