{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAX-D9W"]
[]
[]
[]
[]
["","","","","","EGSAX06DA9W","EGSAX10DA9W"]
["Varmekapacitet","Min.","","","kW","0.85","0.85"]
["","Nom.","","","kW","3.35","5.49"]
["","Max.","","","kW","7.98","9.55"]
["Indgangseffekt","Nom.","","","kW","0.74","1.17"]
["COP","","","","","4.51","4.70"]
["Casing","Colour","","","","Hvid + sort","Hvid + sort"]
["","Materiale","","","","Belagt plademetal"]
["Mål","Enhed","","Højde","mm","1,891","1,891"]
["","","","Bredde","mm","597","597"]
["","","","Dybde","mm","666","666"]
["Vægt","Enhed","","","kg","222","222"]
["Tank","Vandmængde","","","l","180"]
["","Isolering","","Varmetab","kWt/24t","1.2","1.2"]
["","Rustbeskyttelse","","","","Bejdsning","Bejdsning"]
["Kølemiddel","Type","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Belastning","","","kg","1.70","1.70"]
["Driftsområde","Installationsplads","","Min.","°C","5","5"]
["","","","Maks.","°C","35","35"]
["","Saltvandside","","Min.","°C","-10","-10"]
["","","","Maks.","°C","30","30"]
["","Heating","Vandside","Min.","°C","5","5"]
["","","","Max.","°C","65","65"]
["","Varmt vand til beboelse","Vandside","Min.","°C","25","25"]
["","","","Max.","°C","60","60"]
["Rumopvarmning","Vandudgang på 55 °C ved gennemsnitsklima","Generelt","SCOP","","3.77 (1)","4.05 (1)"]
["","","","Seasonal space heating eff. class","","A++","A+++"]
["","Vandudg på 35°C ved gennemsnitsklima","Generelt","SCOP","","5.18 (1)","5.20 (1)"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","A+++","A+++"]
["Power supply","Phase","","","","1~/3~","1~/3~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","230/400","230/400"]
["Strøm","Anbefalede sikringer","","","A","16/32","16/32"]
["Bemærkninger","","","","","(1) - I henhold til EN14825 og EN14511:2018","(1) - I henhold til EN14825 og EN14511:2018"]
["","","","","","(2) - Se tegning over driftsområde: område øget med støtte fra boostervarmer eller backupvarmer","(2) - Se tegning over driftsområde: område øget med støtte fra boostervarmer eller backupvarmer"]