{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W (Archived)"]
["Lydtryk","Nom.","","","dBA","32.0 (6)"]
["Kølemiddel","GWP","","","","2,090"]
["","Opladning","","","kg","1.80"]
["","Type","","","","R-410A"]
["Driftsområde","Installationsplads","","Min.","°C","5.00"]
["","","","Maks.","°C","30.0"]
["","Varme","Vandside","Max.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Saltvandside","","Min.","°C","-5.00"]
["","","","Maks.","°C","20.0"]
["","Varmt vand til beboelse","Vandside","Max.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Indgangseffekt","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Lydeffektniveau","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Mål","Enhed","","Bredde","mm","600"]
["","","","Dybde","mm","728"]
["","","","Højde","mm","1,730"]
["Kabinet","Materiale","","","","Belagt plademetal"]
["","Farve","","","","Hvid"]
["Tank","Vandmængde","","","l","180"]
["","Rustbeskyttelse","","","","Anode"]
["","Isolering","","Varmetab","kWt/24t","1.36 (4)"]
["Vægt","Enhed","","","kg","210"]
["Rumopvarmning","Vandudg på 35°C ved gennemsnitsklima","Generelt","ηs (Effektivitet for rumopvarmning på helårsbasis)","%","194"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","A+++"]
["","","","SCOP","","5.06"]
["","Vandudgang på 55 °C ved gennemsnitsklima","Generelt","Seasonal space heating eff. class","","A++"]
["","","","ηs (Effektivitet for rumopvarmning på helårsbasis)","%","139"]
["","","","SCOP","","3.68"]
["Varmekapacitet","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Max.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Fase","","","","3~"]
["","Navn","","","","9W"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","400"]
["Effekt","Anbefalede sikringer","","","A","25"]
["Bemærkninger","","","","","(1) - EWB/LWB 0 °C/-3 °C - LWC 35 °C (DT=5 °C)"]
["","","","","","(2) - EWB/LWB 0 °C/-3 °C - LWC 45°C (DT=5 °C)"]
["","","","","","(3) - med 40 % propylenglykol"]
["","","","","","(4) - Varmetab ifølge EN12897"]
["","","","","","(5) - med rørføring + PHE + ekstra sikkerhedsvarmer; uden ekspansionskar"]
["","","","","","(6) - Lydeffekten måles via en mikrofon i 1 meters afstand fra enheden. Det er en relativ værdi, som afhænger af afstanden og de akustiske forhold."]
["","","","","","(7) - Via varmepumpe"]
["","","","","","(8) - Via varmepumpe + reservevarmer"]
["","","","","","(9) - Via reservevarmer"]