{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-E"]
[]
[]
[]
[]
["","","","","","EHSHB04P30EF","EHSHB04P30EG","EHSHB08P30EF","EHSHB08P30EG","EHSHB08P50EF","EHSHB08P50EG"]
["Kabinet","Farve","","","","hvid (RAL9016) / sort (RAL9017)","hvid (RAL9016) / sort (RAL9017)","hvid (RAL9016) / sort (RAL9017)","hvid (RAL9016) / sort (RAL9017)","hvid (RAL9016) / sort (RAL9017)","hvid (RAL9016) / sort (RAL9017)"]
["","Materiale","","","","Slagfast polypropylen","Slagfast polypropylen","Slagfast polypropylen","Slagfast polypropylen","Slagfast polypropylen","Slagfast polypropylen"]
["Mål","Enhed","","Højde","mm","1892","1891","1892","1891","1905","1910"]
["","","","Bredde","mm","594","594","594","594","792","792"]
["","","","Dybde","mm","644","644","644","644","812","817"]
["Vægt","Enhed","","","kg","79","80.0","79","80.0","110","104"]
["PED","Kategori","","","","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3"]
["Kølemiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675","675.0","675","675.0","675","675.0"]
["","Belastning","","","kg","1.5","1.50","1.5","1.50","1.5","1.50"]
["Lydeffektniveau","Nom.","","","dBA","39","39","39","39","39","39"]
["Driftsområde","Varme","Vandside","Min.","°C","18","18","18","18","18","18"]
["","","","Max.","°C","65","65","65","65","65","65"]
["","Køle","Omgivende","Min.","°CDB","10","10","10","10","10","10"]
["","","Vandside","Min.","°C","5","5","5","5","5","5"]
["","","","Max.","°C","22","22","22","22","22","22"]
["Strømforsyning","Fase","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50","50","50","50"]
["","Strømspænding","","","V","230","230","230","230","230","230"]
["Bemærkninger","","","","","(1) - Varmetab ifølge EN12897","(1) - Varmetab ifølge EN12897","(1) - Varmetab ifølge EN12897","(1) - Varmetab ifølge EN12897","(1) - Varmetab ifølge EN12897","(1) - Varmetab ifølge EN12897"]