{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3 / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHSX04P30DA3 / ERGA04EAV3","EHSX04P50DA3 / ERGA04EAV3"]
["Opvarmning af varmt brugsvand","Generelt","","Erklæret belastningsprofil","","L","XL"]
["","Gennemsnitsklima","","Energieffektivitetsklasse for vandopvarmning","","A+","A"]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)"]
["Indendørs enhed","","","","","EHSX04P30DA3","EHSX04P50DA3"]
["Rumopvarmning","Vandudgang på 55 °C ved gennemsnitsklima","Generelt","Seasonal space heating eff. class","","A++","A++"]
["","","","ηs (Effektivitet for rumopvarmning på helårsbasis)","%","129","129"]
["","","","SCOP","","3.29","3.29"]
["Kølekapacitet","Nom.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)"]
["Varmekapacitet","Nom.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)"]
["Indgangseffekt","Køle","","Nom.","kW","0.810 (1), 1.36 (2)","0.810 (1), 1.36 (2)"]
["","Varme","","Nom.","kW","0.840 (1), 1.26 (2)","0.840 (1), 1.26 (2)"]
["Bemærkninger","","","","","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]