{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-E / ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","EHSXB08P30EF / ERGA08EAV3H7","EHSXB08P50EF / ERGA08EAV3H7"]
["Indendørs enhed","","","","","EHSXB08P30EF","EHSXB08P50EF"]
["Varmekapacitet","Nom.","","","kW","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Kølekapacitet","Nom.","","","kW","6.25 (1), 5.44 (2)","6.25 (1), 5.44 (2)"]
["Indgangseffekt","Varme","","Nom.","kW","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["","Køle","","Nom.","kW","1.16 (1), 1.73 (2)","1.16 (1), 1.73 (2)"]
["COP","","","","","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["EER","","","","","5.40 (1), 3.14 (2)","5.40 (1), 3.14 (2)"]
["Opvarmning af varmt brugsvand","Generelt","","Erklæret belastningsprofil","","L","XL"]
["","Gennemsnitsklima","","Energieffektivitetsklasse for vandopvarmning","","A+","A+"]
["Rumopvarmning","Vandudgang på 55 °C ved gennemsnitsklima","Generelt","SCOP","","3.35","3.35"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","A++","A++"]
["","Vandudgang på 35°C ved gennemsnitsklima","Generelt","SCOP","","4.61","4.61"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","A+++","A+++"]
["Bemærkninger","","","","","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]