{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-UE6V / ERGA-EVH"]
[]
[]
[]
[]
["","","","","","EHVH08SU18EA6V / ERGA06EAV3H","EHVH08SU18EJ6V / ERGA06EAV3H","EHVH08SU23EA6V / ERGA06EAV3H","EHVH08SU23EJ6V / ERGA06EAV3H"]
["Varmekapacitet","Nom.","","","kW","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)"]
["Indgangseffekt","Varme","","Nom.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)"]
["Strømforbrug","Opvarmning af brugsvand fra 10°C til 50 °C","","Nom.","kWh","2.48","2.48","3.01","3.01"]
["Opvarmningstid fra 10°C til 50 °C","tim","","","","1t28min","1t28min","1t40min","1t40min"]
["COP","","","","","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)"]
["Opvarmning af varmt brugsvand","Generelt","","Erklæret belastningsprofil","","L","L","XL","XL"]
["","Gennemsnitsklima","","Energieffektivitetsklasse for vandopvarmning","","A+","A+","A+","A+"]
["Rumopvarmning","Vandudgang på 55 °C ved gennemsnitsklima","Generelt","SCOP","","3.26","3.26","3.26","3.26"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","A++","A++","A++","A++"]
["","Vandudgang på 35°C ved gennemsnitsklima","Generelt","SCOP","","4.47","4.47","4.47","4.47"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","A+++","A+++","A+++","A+++"]
["Bemærkninger","","","","","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]