{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-E6V / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHVZ04S18EA6V / ERGA04EAV3"]
["Varmekapacitet","Nom.","","","kW","4.30 (1), 4.60 (2)"]
["Indgangseffekt","Varme","","Nom.","kW","0.850 (1), 1.26 (2)"]
["Strømforbrug","Opvarmning af brugsvand fra 10°C til 50 °C","","Nom.","kWh","2.48"]
["Opvarmningstid fra 10°C til 50 °C","tim","","","","1t28min"]
["COP","","","","","5.10 (1), 3.65 (2)"]
["Opvarmning af varmt brugsvand","Generelt","","Erklæret belastningsprofil","","L"]
["","Gennemsnitsklima","","Energieffektivitetsklasse for vandopvarmning","","A+"]
["Rumopvarmning","Vandudgang på 55 °C ved gennemsnitsklima","Generelt","SCOP","","3.26"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","A++"]
["","Vandudgang på 35°C ved gennemsnitsklima","Generelt","SCOP","","4.48"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","A+++"]
["Energieffektivitetsklasse","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Bemærkninger","","","","","(1) - Betingelse 1: køle Ta 35°C - LWE 18℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Betingelse 2: køle Ta 35°C - LWE 7℃ (DT = 5°C); varmeTa DB/WB 7°C/6°C - LWC 45℃ (DT = 5°C)"]