{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK08-10AW1"]
[]
[]
[]
[]
["","","","","","EPSK08ARW1","EPSK10ARW1"]
["Mål","Enhed","","Højde","mm","1123","1123"]
["","","","Bredde","mm","1330","1330"]
["","","","Dybde","mm","604","604"]
["Vægt","Enhed","","","kg","178","178"]
["Ventilator","Luftmængde","Varme","Høj","m³/min","75.7","75.7"]
["","","Køle","Høj","m³/min","75.7","75.7"]
["Driftsområde","Køle","","Min.","°CDB","10","10"]
["","","","Maks.","°CDB","43","43"]
["","Varmt vand til beboelse","","Min.","°CDB","-28","-28"]
["","Varmt brugsvand","","Maks.","°CDB","40","40"]
["Lydeffektniveau","Varme","","Nom.","dBA","45 (1)","47 (1)"]
["","Køle","","Nom.","dBA","53 (2)","53.2 (2)"]
["Lydtryk","Varme","","Nom.","dBA","32.4 (1)","32.8 (1)"]
["","Køle","","Nom.","dBA","37.2 (2)","37.3 (2)"]
["Kølemiddel","Type","","","","R-290","R-290"]
["","GWP","","","","3","3"]
["","Påfyldning","","","tCO2Eq","0.003","0.003"]
["","Belastning","","","kg","1","1"]
["Rørtilslutninger","Niveauforskel","IU - OU","Max.","m","10","10"]
["Strømforsyning","Navn","","","","W1","W1"]
["","Fase","","","","3~","3~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","400","400"]
["Strøm","Anbefalede sikringer","","","A","16","16"]
["Bemærkninger","","","","","(1) - Målt ved LWC 47-55 °C; Ta DB/WB 7 °C/6 °C.","(1) - Målt ved LWC 47-55 °C; Ta DB/WB 7 °C/6 °C."]
["","","","","","(2) - Målt ved LWC 12-7 °C; Ta 35°C.","(2) - Målt ved LWC 12-7 °C; Ta 35°C."]
["","","","","","(3) - 1 1/4\" rørføring på installationssted","(3) - 1 1/4\" rørføring på installationssted"]
["","","","","","(4) - 1 1/2\" rørføring på installationssted","(4) - 1 1/2\" rørføring på installationssted"]