{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPVX10UA4V / EPSK08-10AW1"]
[]
[]
[]
[]
["","","","","","EPVX10SU18AJ4V / EPSK08ARW1","EPVX10SU23AJ4V / EPSK08ARW1","EPVX10SU18AJ4V / EPSK10ARW1","EPVX10SU23AJ4V / EPSK10ARW1"]
["Varmekapacitet","Nom.","","","kW","7.62 (1)","7.62 (1)","8.11 (1)","8.11 (1)"]
["Kølekapacitet","Nom.","","","kW","6.89 (2), 6.37 (3)","6.89 (2), 6.37 (3)","7.84 (2), 6.37 (3)","7.84 (2), 6.37 (3)"]
["Indgangseffekt","Varme","","Nom.","kW","1.52 (1)","1.52 (1)","1.64 (1)","1.64 (1)"]
["","Køle","","Nom.","kW","1.85 (2), 1.13 (3)","1.85 (2), 1.13 (3)","2.17 (2), 1.13 (3)","2.17 (2), 1.13 (3)"]
["Strømforbrug","Opvarmning af brugsvand fra 10°C til 50 °C","","Nom.","kWh","2.35","2.89","2.35","2.89"]
["Opvarmningstid fra 10°C til 50 °C","tim","","","","1t 27min","1t 58min","1t 27min","1t 58min"]
["COP","","","","","5.01 (1)","5.01 (1)","4.94 (1)","4.94 (1)"]
["EER","","","","","3.73 (2), 5.63 (3)","3.73 (2), 5.63 (3)","3.62 (2), 5.63 (3)","3.62 (2), 5.63 (3)"]
["Opvarmning af varmt brugsvand","Generelt","","Erklæret belastningsprofil","","L","L","L","L"]
["","Gennemsnitsklima","","Energieffektivitetsklasse for vandopvarmning","","A+","A+","A+","A+"]
["Rumopvarmning","Vandudgang på 55 °C ved gennemsnitsklima","Generelt","SCOP","","3.94","3.94","3.99","3.99"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","A+++","A+++","A+++","A+++"]
["","Vandudgang på 35°C ved gennemsnitsklima","Generelt","SCOP","","5.14","5.14","5.14","5.14"]
["","","","Klasse for effektivitet for rumopvarmning på helårsbasis","","A+++","A+++","A+++","A+++"]
["Bemærkninger","","","","","(1) - Betingelse: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Betingelse: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Betingelse: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Betingelse: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Køle: EW 12℃; LW 7℃ omgivende forhold: 35 °CDB","(2) - Køle: EW 12℃; LW 7℃ omgivende forhold: 35 °CDB","(2) - Køle: EW 12℃; LW 7℃ omgivende forhold: 35 °CDB","(2) - Køle: EW 12℃; LW 7℃ omgivende forhold: 35 °CDB"]
["","","","","","(3) - Køle: EW 23℃; LW 18℃ omgivende forhold: 35 °CDB","(3) - Køle: EW 23℃; LW 18℃ omgivende forhold: 35 °CDB","(3) - Køle: EW 23℃; LW 18℃ omgivende forhold: 35 °CDB","(3) - Køle: EW 23℃; LW 18℃ omgivende forhold: 35 °CDB"]