{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","ERGA08EAV3H7"]
["Mål","Enhed","","Højde","mm","740"]
["","","","Bredde","mm","884"]
["","","","Dybde","mm","388"]
["Vægt","Enhed","","","kg","58.5"]
["Driftsområde","Køle","","Min.","°CDB","10"]
["","","","Maks.","°CDB","43"]
["","Varmt vand til beboelse","","Min.","°CDB","-25"]
["","Varmt brugsvand","","Maks.","°CDB","35"]
["Lydeffektniveau","Varme","","Nom.","dBA","62 (1)"]
["","Køle","","Nom.","dBA","62 (1)"]
["Lydtryk","Varme","","Nom.","dBA","49 (1)"]
["","Køle","","Nom.","dBA","50 (1)"]
["Kølemiddel","Type","","","","R-32"]
["","GWP","","","","675.0"]
["","Påfyldning","","","tCO2Eq","1.01"]
["","Belastning","","","kg","1.50"]
["Rørtilslutninger","Flydende","","UD","mm","6"]
["","Gas","","UD","mm","15.9"]
["","Dræn","","UD","mm","18"]
["","Niveauforskel","IU - OU","Max.","m","30.0"]
["","Varmeisolering","","","","Både væske- og gasrør"]
["Strømforsyning","Navn","","","","V3"]
["","Fase","","","","1 N~"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","230"]
["Strøm","Anbefalede sikringer","","","A","25"]
["Bemærkninger","","","","","(1) - Køling Ta 35 °C - LWE 18 °C ( DT = 5 °C ) - Opvarmning Ta DB/WB 7 °C/6 °C - LWC 35 ℃ ( DT = 5 °C )"]