{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB-D"]
[]
[]
[]
[]
["","","","","","ETSHB16P30DA","ETSHB16P50DA"]
["Lydtryk","Nom.","","","dBA","32.8","32.8"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","10","10"]
["","","Vandside","Max.","°C","22","22"]
["","","","Min.","°C","5","5"]
["","Varme","Vandside","Max.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Lydeffektniveau","Nom.","","","dBA","45.6","45.6"]
["Mål","Enhed","","Bredde","mm","590","785"]
["","","","Dybde","mm","615","785"]
["","","","Højde","mm","1,891","1,896"]
["Kabinet","Materiale","","","","Slagfast polypropylen","Slagfast polypropylen"]
["","Farve","","","","Traffic hvid (RAL9016) / Mørkegrå (RAL7011)","Traffic hvid (RAL9016) / Mørkegrå (RAL7011)"]
["PED","Kategori","","","","Art4.3","Art4.3"]
["Vægt","Enhed","","","kg","75","96"]
["Power supply","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","230","230"]
["Elvarmer","Strømforsyning","","Frekvens","Hz","50","50"]
["","","","Navn","","3V / 9W","3V / 9W"]
["","","","Fase","","1~ / 3~","1~ / 3~"]
["Bemærkninger","","","","","(1) - Varmetab ifølge EN12897","(1) - Varmetab ifølge EN12897"]
["","","","","","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C"]
["","","","","","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 °C","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 °C"]
["","","","","","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 °C","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 °C"]