{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSXB16E"]
[]
[]
[]
[]
["","","","","","ETSXB16P30EF","ETSXB16P50EF"]
["Kabinet","Farve","","","","hvid (RAL9016) / sort (RAL9017)","hvid (RAL9016) / sort (RAL9017)"]
["","Materiale","","","","Slagfast polypropylen","Slagfast polypropylen"]
["Mål","Enhed","","Højde","mm","1,892","1,910"]
["","","","Bredde","mm","594","792"]
["","","","Dybde","mm","644","816"]
["Vægt","Enhed","","","kg","76","100"]
["Lydeffektniveau","Nom.","","","dBA","45.6","45.6"]
["Lydtryk","Nom.","","","dBA","32.8","32.8"]
["Driftsområde","Varme","Vandside","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["","Køle","Omgivende","Min.","°CDB","0 (2)","0 (2)"]
["","","Vandside","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["Power supply","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","230","230"]
["Bemærkninger","","","","","(1) - Varmetab ifølge EN12897","(1) - Varmetab ifølge EN12897"]
["","","","","","(2) - Se tegninger over driftsgrænser","(2) - Se tegninger over driftsgrænser"]