{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Kabinet","Farve","","","","Hvid","Hvid"]
["","Materiale","","","","Plast","Plast"]
["Mål","Enhed","","Højde","mm","290","340"]
["","","","Bredde","mm","1050","1200"]
["","","","Dybde","mm","269","262"]
["Vægt","Enhed","","","kg","14","18"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","16.2","23"]
["","","Køling","Mellem","m³/min","13.4","21.1"]
["","","","Lav","m³/min","12.1","18.7"]
["","","Varme","Høj","m³/min","16.9","23"]
["","","Opvarmning","Mellem","m³/min","14.2","20.9"]
["","","Varme","Lav","m³/min","12.7","18.7"]
["Lydeffekt","Køling","","","dBA","61","65"]
["","Opvarmning","","","dBA","61","65"]
["Lydtryk","Køle","","Høj","dBA","45","49"]
["Lydtryksniveau","Køling","","Mellem","dBA","42","45"]
["Lydtryk","Køle","","Lav","dBA","40","41"]
["","Varme","","Høj","dBA","45","49"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","42","45"]
["Lydtryk","Varme","","Lav","dBA","40","41"]
["Rørtilslutninger","Flydende","","UD","mm","9.52","9.52"]
["","Gas","","UD","mm","15.9","15.9"]
["","Dræn","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Strømforsyning","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","220-240","220-240"]
["Standardtilbehør","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Bemærkninger","","","","","(1) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["Standardtilbehør","Screw cover","","","","","3"]