{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXS-L"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RXS50L2V1B","FBA60A2VEB9 / RXS60L2V1B"]
["Kølekapacitet","Nom.","","kW","","5.70"]
["Nominel effektivitet","Årligt energiforbrug","","kWh","","826"]
["","EER","","","","3.45"]
["","COP","","","","37.10"]
["","Direktiv om energimærkning","Køling","","","A"]
["","","Opvarmning","","","A"]
["Varmekapacitet","Nom.","","kW","","7.00"]
["Bemærkninger","","","","","(1) - Nominel kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","","(3) - Se separat tegning for driftsområde"]
["","","","","","(4) - Se særskilte tegninger med de elektriske data"]
["Udendørs enhed","","","","RXS50L2V1B"]
["Kølekapacitet","Nom.","","kW","5.00"]
["Varmekapacitet","Nom.","","kW","5.50"]
["Nominel effektivitet","EER","","","3.52"]
["","COP","","","38.30"]
["","Årligt energiforbrug","","kWh","710"]
["","Direktiv om energimærkning","Køling","","A"]
["","","Opvarmning","","A"]
["Rumkøling","Energieffektivitetsklasse","","","A++"]
["","Kapacitet","Pdesign","kW","5.00"]
["","SEER","","","6.21"]
["","Årligt energiforbrug","","kWh/a","282"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A+"]
["","Kapacitet","Pdesign","kW","4.40"]
["","SCOP/A","","","4.06"]
["","Pdh varmekapacitet ved -10°","","kW","3.73"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/a","1517"]
["Energieffektivitetsklasse","","","","A+++ ~ D"]