{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZAG-B"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RZAG35B5V1B","FBA35A2VEB9 / RZAG35B5V1B","FBA60A2VEB9 / RZAG50B5V1B","FBA50A2VEB9 / RZAG50B5V1B","FBA71A2VEB9 / RZAG60B5V1B","FBA60A2VEB9 / RZAG60B5V1B"]
["Kølekapacitet","Min.","","kW","1.6","1.6","1.7","1.7","1.7","1.7"]
["","Nom.","","kW","3.5","3.5","5","5","6","6"]
["","Max.","","kW","5","5","6","6","7","7"]
["Varmekapacitet","Min.","","kW","1.4","1.4","1.7","1.7","1.7","1.7"]
["","Nom.","","kW","4","4","6","6","7","7"]
["","Max.","","kW","5","5","6","6","7.5","7.5"]
["Nominel effektivitet","EER","","","4.62","4.5","4.11","4","4.31","4.05"]
["","COP","","","4.44","4.4","3.97","3.8","3.87","3.8"]
["","Årligt energiforbrug","","kWt","379","389","608","625","696","741"]
["","Direktiv om energimærkning","Køling","","A","A","A","A","A","A"]
["","","Opvarmning","","A","A","A","A","A","C"]
["Rumkøling","Energieffektivitetsklasse","","","A++","A++","A++","A++","A++","A++"]
["","Kapacitet","Pdesign","kW","3.5","3.5","5","5","6","6"]
["","SEER","","","6.17","6.12","6.63","6.3","6.25","6.15"]
["","Årligt energiforbrug","","kWh/å","199","200","264","278","336","341"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A+","A+","A+","A+","A+","A+"]
["","Kapacitet","Pdesign","kW","4.2","4.2","4.3","4.3","4.5","4.5"]
["","SCOP/A","","","4.14","4.1","4.28","4.1","4.18","4.1"]
["","Pdh varmekapacitet ved -10°","","kW","3.51","3.49","3.75","3.65","3.86","3.85"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/å","1420","1434","1406","1469","1508","1537"]
["Energieffektivitetsklasse","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]