{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FBA71A2VEB / AZAS71M2V1B (Archived)"]
["Outdoor unit","","","","AZAS71M2V1B"]
["Kølekapacitet","Nom.","","kW","6.80"]
["Varmekapacitet","Nom.","","kW","7.50"]
["Rumkøling","Energieffektivitetsklasse","","","A"]
["","Kapacitet","Pdesign","kW","6.80"]
["","SEER","","","5.57"]
["","Årligt energiforbrug","","kWh/å","427"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A"]
["","Kapacitet","Pdesign","kW","4.50"]
["","SCOP/A","","","3.81"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/å","1654"]
["Bemærkninger","","","","(1) - Køling: T2: indendørs temp. 26,6 °CDB, 19,4 °CWB, udendørs temp. 48°CDB [Btu/hr/W]"]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]