{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["Lydtryk","Varme","","Høj","dBA","37.0","37.0","31.0","31.0"]
["","","","Mellem","dBA","34.0","34.0","28.0","28.0"]
["","","","Lav","dBA","29.0","29.0","25.0","25.0"]
["","Køle","","Mellem","dBA","32.0","32.0","28.0","28.0"]
["","","","Lav","dBA","29.0","29.0","25.0","25.0"]
["","","","Høj","dBA","35.0","35.0","30.0","30.0"]
["Standardtilbehør","Betjeningsvejledning","","","","1","1","1","1"]
["","Installationsvejledning","","","","1","1","1","1"]
["","Afløbsslange","","","","1","1","1","1"]
["","Metalklemme til afløbsslange","","","","1","1","1","1"]
["","Spændeskive til ophængsbeslag","","","","8","8","8","8"]
["","Skruer","","","","40","40","40","40"]
["","Isolering til fitting","","","","2","2","2","2"]
["","Forseglingspuder","","","","5","5","5","5"]
["","Klemmer","","","","4","4","4","4"]
["Control systems","Fortrådet fjernbetjening","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Rørtilslutninger","Flydende","","UD","mm","6.35","6.35","6.35","9.52"]
["","Gas","","UD","mm","9.52","12.70","12.70","15.90"]
["","Dræn","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Lydeffektniveau","Køling","","","dBA","60","60","56","56"]
["Mål","Enhed","","Bredde","mm","700","700","1,000","1,000"]
["","","","Dybde","mm","800","800","800","800"]
["","","","Højde","mm","245","245","245","245"]
["Kabinet","Material","","","","Galvaniseret stålplade","Galvaniseret stålplade","Galvaniseret stålplade","Galvaniseret stålplade"]
["","Farve","","","","Ikke malet (galvaniseret)","Ikke malet (galvaniseret)","Ikke malet (galvaniseret)","Ikke malet (galvaniseret)"]
["Vægt","Enhed","","","kg","28.0","28.0","35.0","35.0"]
["Ventilator","Udvendigt statisk tryk","","Høj","Pa","150","150","150","150"]
["","","","Nom.","Pa","30","30","30","30"]
["","Luftmængde","Varme","Høj","m³/min","15.0","15.0","18.0","18.0"]
["","","","Lav","m³/min","10.5","10.5","12.5","12.5"]
["","","","Mellem","m³/min","12.5","12.5","15.0","15.0"]
["","","Cooling","Lav","m³/min","10.5","10.5","12.5","12.5"]
["","","","Mellem","m³/min","12.5","12.5","15.0","15.0"]
["","","","Høj","m³/min","15.0","15.0","18.0","18.0"]
["Dræn-op højde","mm","","","","625","625","625","625"]
["Power supply","Fase","","","","1~","1~","1~","1~"]
["","Frekvens","","","Hz","50/60","50/60","50/60","50/60"]
["","Strømspænding","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Bemærkninger","","","","","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer."]
["","","","","","(2) - Se særskilte tegninger med de elektriske data","(2) - Se særskilte tegninger med de elektriske data","(2) - Se særskilte tegninger med de elektriske data","(2) - Se særskilte tegninger med de elektriske data"]