{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RXS-L3"]
[]
[]
[]
[]
["","","","","FBQ35C8VEB / RXS35L3V1B"]
["Kølekapacitet","Min.","","kW","1.4"]
["","Max.","","kW","3.9"]
["","Nom.","","kW","3.40 (2)"]
["Piping connections","Flydende","UD","mm","6.35"]
["","Gas","UD","mm","9.5"]
["","Dræn","UD","mm","VP25 (ekstern dia.32, intern dia. 25)"]
["Nominel effektivitet","Årligt energiforbrug","","kWt","459"]
["","EER","","","3.70"]
["","COP","","","3.60"]
["","Direktiv om energimærkning","Køling","","A"]
["","","Opvarmning","","B"]
["Varmekapacitet","Nom.","","kW","4.00 (2)"]
["","Min.","","kW","1.3"]
["","Max.","","kW","5.0"]
["Bemærkninger","","","","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU"]
["","","","","(2) - Nominel effektivitet: Køling ved 35°/27° nominel belastning, opvarmning ved 7°/20° nominel belastning"]
["","","","","(3) - 220V"]
["","","","","(4) - 230V"]
["","","","","(5) - 240V"]