{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":14,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBQ35D2VEB / FBQ35D2VEB / RZQSG71L3V1B","FBQ71D2VEB / RZQSG71L3V1B (Preliminary)","FBQ100D2VEB / RZQSG100L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQSG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQSG100L9V1B","FBQ125D2VEB / RZQSG125L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQSG125L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQSG125L9V1B","FBQ60D2VEB / FBQ60D2VEB / RZQSG125L9V1B","FBQ140D2VEB / RZQSG140L9V1B"]
["Rumkøling","SEER","","","5.10","5.84","5.61","5.10","5.10","5.47","4.80","4.80","4.80"]
["","Årligt energiforbrug","","kWh/a","467","408","593","652","652","768","875","875","875"]
["","Kapacitet","Pdesign","kW","6.80","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Energieffektivitetsklasse","","","A","A+","A+","A","A","A","B","B","B"]
["Rumopvarmning (gennemsnitsklima)","Kapacitet","Pdesign","kW","6.00","6.00","7.60","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","4.10","4.15","3.80","3.80","4.01","3.80","3.80","3.80"]
["","Energieffektivitetsklasse","","","A","A+","A+","A","A","A+","A","A","A"]
["","Årligt energiforbrug","","kWh/a","2,211","2,049","2,564","2,800","2,800","2,653","2,800","2,800","2,800"]
["Bemærkninger","","","","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","","","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","","","","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU"]
["","","","","(2) - Nominel effektivitet: Køling ved 35°/27° nominel belastning, opvarmning ved 7°/20° nominel belastning","(2) - Nominel effektivitet: Køling ved 35°/27° nominel belastning, opvarmning ved 7°/20° nominel belastning","(2) - Nominel effektivitet: Køling ved 35°/27° nominel belastning, opvarmning ved 7°/20° nominel belastning","","","(2) - Nominel effektivitet: Køling ved 35°/27° nominel belastning, opvarmning ved 7°/20° nominel belastning","","","","(2) - Nominel effektivitet: Køling ved 35°/27° nominel belastning, opvarmning ved 7°/20° nominel belastning"]
["Kølekapacitet","Nom.","","kW","","6.8","9.5 (2)","","","12.0 (2)","","","","13.4 (2)"]
["Nominel effektivitet","Årligt energiforbrug","","kWt","","1,030","1,418","","","1,858"]
["","EER","","","","3.30","3.35 (1)","","","3.23 (1)","","","","3.06 (1)"]
["","COP","","","","3.81","3.67 (1)","","","3.63 (1)","","","","3.40 (1)"]
["","Direktiv om energimærkning","Køling","","","A","A","","","A"]
["","","Opvarmning","","","A","A","","","A"]
["Varmekapacitet","Nom.","","kW","","7.5","10.80 (2)","","","13.50 (2)","","","","15.50 (2)"]
["Bemærkninger","","","","","","(3) - Årligt energiforbrug ifølge Direktivet for energimærkning 2002/31/EC","","","(3) - Årligt energiforbrug ifølge Direktivet for energimærkning 2002/31/EC"]
["","","","","","","(4) - SEER og SCOP er i overensstemmelse med EN 14825","","","(4) - SEER og SCOP er i overensstemmelse med EN 14825"]
["","","","","","","","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","(1) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU"]