{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D"]
[]
[]
[]
[]
["","","","","","FBQ35D2VEB","FBQ50D2VEB","FBQ60D2VEB","FBQ71D2VEB","FBQ100D2VEB","FBQ125D2VEB","FBQ140D2VEB"]
["Lydtryk","Varme","","Høj","dBA","37","37","31","31.0","36.0","38.0","38"]
["","","","Mellem","dBA","34","34","28","28.0","33.0","35.0","35"]
["","","","Lav","dBA","29","29","25","25.0","30.0","32.0","32"]
["","Køle","","Mellem","dBA","32","32","28","28.0","32.0","35.0","35"]
["","","","Lav","dBA","29","29","25","25.0","30.0","32.0","32"]
["","","","Høj","dBA","35","35","30","30.0","34.0","37.0","37"]
["Standardtilbehør","Betjeningsvejledning","","","","1","1","1","1","1","1","1"]
["","Installationsvejledning","","","","1","1","1","1","1","1","1"]
["","Afløbsslange","","","","1","1","1","1","1","1","1"]
["","Metalklemme til afløbsslange","","","","1","1","1","1","1","1","1"]
["","Spændeskive til ophængsbeslag","","","","8","8","8","8","8","8","8"]
["","Skruer","","","","40","40","40","40","40","40","40"]
["","Isolering til fitting","","","","2","2","2","2","2","2","2"]
["","Forseglingspude","","","","5","5","5","5","5","5","5"]
["","Forseglingspuder","","","","","","","5","5","5","5"]
["","Klemmer","","","","4","4","4","4","4","4","4"]
["Kølemiddel","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Styresystemer","Fortrådet fjernbetjening","","","","","","","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528"]
["","Infrared remote control","","","","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Rørføringsforbindelser","Flydende","","UD","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gas","","UD","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Dræn","","","","VP20 (I.D. 20/U.D. 26), afløbshøjde 625 mm","VP20 (I.D. 20/U.D. 26), afløbshøjde 625 mm","VP20 (I.D. 20/U.D. 26), afløbshøjde 625 mm","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Køling","","","dBA","60","60","56","56","58","62","62"]
["Mål","Enhed","","Bredde","mm","700","700","1,000","1,000","1,400","1,400","1,400"]
["","","","Dybde","mm","800","800","800","800","800","800","800"]
["","","","Højde","mm","245","245","245","245","245","245","245"]
["Kabinet","Materiale","","","","Galvaniseret stålplade","Galvaniseret stålplade","Galvaniseret stålplade","Galvaniseret stålplade","Galvaniseret stålplade","Galvaniseret stålplade","Galvaniseret stålplade"]
["","Farve","","","","Ikke malet (galvaniseret)","Ikke malet (galvaniseret)","Ikke malet (galvaniseret)","Ikke malet (galvaniseret)","Ikke malet (galvaniseret)","Ikke malet (galvaniseret)","Ikke malet (galvaniseret)"]
["Vægt","Enhed","","","kg","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Ventilator","Udvendigt statisk tryk","","Høj","Pa","150","150","150","150","150","150","150"]
["","","","Nom.","Pa","30","30","30","30","40","50","50"]
["","Luftmængde","Varme","Høj","m³/min","","","","","29.0","34.0","34.0"]
["","","","Lav","m³/min","","","","","23.0","23.5","23.5"]
["","","","Mellem","m³/min","","","","","26.0","29.0","29.0"]
["","","Køle","Lav","m³/min","","","","","23.0","23.5","23.5"]
["","","","Mellem","m³/min","","","","","26.0","29.0","29.0"]
["","","","Høj","m³/min","","","","","29.0","34.0","34.0"]
["Dræn-op højde","mm","","","","625","625","625","625","625","625","625"]
["Power supply","Fase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvens","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Navn","","","","VE","VE","VE","VE","VE","VE","VE"]
["","Strømspænding","","","V","220-240","220-240","220-240","220-240/220","220-240/220","220-240/220","220-240/220"]
["Bemærkninger","","","","","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer."]