{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RXS-L3"]
[]
[]
[]
[]
["","","","","FCAG35AVEB / RXS35L3V1B"]
["Kølekapacitet","Nom.","","kW","3.40"]
["Space cooling","SEER","","","6.35"]
["","Årligt energiforbrug","","kWh/å","193"]
["","Kapacitet","Pdesign","kW","3.50"]
["","Energieffektivitetsklasse","","","A++"]
["Rumopvarmning (gennemsnitsklima)","Kapacitet","Pdesign","kW","3.32"]
["","SCOP/A","","","4.90"]
["","Energieffektivitetsklasse","","","A++"]
["","Årligt energiforbrug","","kWh/å","949"]
["Rørtilslutninger","Flydende","OD","mm","6.35"]
["","Gas","UD","mm","9.50"]
["","Dræn","OD","mm","VP25 (ekstern dia.32, intern dia. 25)"]
["Nominel effektivitet","EER","","","3.74"]
["","Årligt energiforbrug","","kWt","455"]
["","COP","","","3.50"]
["","Direktiv om energimærkning","Køling","","A"]
["","","Opvarmning","","B"]
["Varmekapacitet","Nom.","","kW","4.20"]
["Bemærkninger","","","","(1) - Nominel kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Se separat tegning for driftsområde"]
["","","","","(4) - Se særskilte tegninger med de elektriske data"]