{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":13,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG100L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQSG125L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQSG100L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQSG125L8Y1B","FCAG100AVEB / RZQSG100L8Y1B","FCAG125AVEB / RZQSG125L8Y1B","FCAG140AVEB / RZQSG140L7Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG140L7Y1B"]
["Energieffektivitetsklasse","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Kølekapacitet","Nom.","","kW","","","","","","9.50 (1)","12.0 (1)","13.4 (1)","13.4 (1)"]
["Rumkøling","SEER","","","","","","","","6.50","5.30"]
["","Årligt energiforbrug","","kWh/å","","","","","","512","793"]
["","Kapacitet","Pdesign","kW","","","","","","9.50","12.0"]
["","Energieffektivitetsklasse","","","","","","","","A++","A"]
["Rumopvarmning (gennemsnitsklima)","Kapacitet","Pdesign","kW","","","","","","7.60","8.03"]
["","SCOP/A","","","","","","","","4.10","4.01"]
["","Energieffektivitetsklasse","","","","","","","","A+","A+"]
["","Årligt energiforbrug","","kWh/å","","","","","","2,596","2,804"]
["Nominel effektivitet","Årligt energiforbrug","","kWh","","","","","","1,440","1,870"]
["","EER","","","","","","","","3.30 (3)","3.21 (3)","2.40 (3)","4.20 (3)"]
["","COP","","","","","","","","3.54 (3)","3.41 (3)","3.41 (3)"]
["","Direktiv om energimærkning","Køling","","","","","","","A","A"]
["","","Opvarmning","","","","","","","A","B"]
["Varmekapacitet","Nom.","","kW","","","","","","10.8 (2)","13.5 (2)","15.5 (2)","15.5 (2)"]
["Bemærkninger","","","","","","","","","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB; tilsvarende rørlængde: 7,5 m, niveauforskel: 0m","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB; tilsvarende rørlængde: 7,5 m, niveauforskel: 0m","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB; tilsvarende rørlængde: 7,5 m, niveauforskel: 0m","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB; tilsvarende rørlængde: 7,5 m, niveauforskel: 0m"]
["","","","","","","","","","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 7,5 m, niveauforskel: 0m","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 7,5 m, niveauforskel: 0m","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 7,5 m, niveauforskel: 0m","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 7,5 m, niveauforskel: 0m"]
["","","","","","","","","","(3) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","(3) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","(3) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU","(3) - EER/COP i overensstemmelse med Eurovent 2012, kun til brug uden for EU"]