{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RXS50L2V1B","FCAG60BVEB / RXS60L2V1B"]
["Kølekapacitet","Nom.","","kW","5.00","5.70"]
["Varmekapacitet","Nom.","","kW","6.00","7.00"]
["Nominel effektivitet","Årligt energiforbrug","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","EER","","","3.55","3.48"]
["","Direktiv om energimærkning","Køling","","A","A"]
["","","Opvarmning","","A","B"]
["Rørtilslutninger","Dræn","UD","mm","VP25 (ekstern dia.32, intern dia. 25)","VP25 (ekstern dia.32, intern dia. 25)"]
["","Gas","UD","mm","12.70","12.70"]
["","Flydende","UD","mm","6.35","6.35"]
["Bemærkninger","","","","(1) - Under normal drift: +22 °C / + 32 °C","(1) - Under normal drift: +22 °C / + 32 °C"]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Se separat tegning for driftsområde","(3) - Se separat tegning for driftsområde"]
["","","","","(4) - Se særskilte tegninger med de elektriske data","(4) - Se særskilte tegninger med de elektriske data"]