{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":23,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["Kølekapacitet","Nom.","","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["Varmekapacitet","Nom.","","kW","","","","","","","","","","","","","","","","","","7.50","15.50"]
["Nominel effektivitet","EER","","","","","","","","","","","","","","","","3.39","3.30","3.30","3.30","3.39","2.50"]
["","COP","","","","","","","","","","","","","","","","","","","","3.97","3.61"]
["","Årligt energiforbrug","","kWh","","","","","","","","","","","","","","","","","","1,003"]
["","Direktiv om energimærkning","Køling","","","","","","","","","","","","","","","","","","","A"]
["","","Opvarmning","","","","","","","","","","","","","","","","","","","A"]
["Rumkøling","Energieffektivitetsklasse","","","","","","","","","","","","","","","","A++","A","A","A","A++"]
["","Kapacitet","Pdesign","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["","SEER","","","","","","","","","","","","","","","","6.80","5.10","5.10","5.10","6.72","6.44"]
["","Årligt energiforbrug","","kWh/a","","","","","","","","","","","","","","350","467","467","467","355","1,249"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","","","","","","","","","","","","","","A+","A","A","A","A+"]
["","Kapacitet","Pdesign","kW","","","","","","","","","","","","","","6.33","6.00","6.00","6.00","6.33","11.56"]
["","SCOP/A","","","","","","","","","","","","","","","","4.20","3.80","3.80","3.80","4.20","4.27"]
["","Årligt energiforbrug","","kWh/a","","","","","","","","","","","","","","2,110","2,211","2,211","2,211","2,110","3,795"]
["Bemærkninger","","","","","","","","","","","","","","","","","(1) - Se separat tegning for driftsområde","(1) - Se separat tegning for driftsområde","(1) - Se separat tegning for driftsområde","(1) - Nominel kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m.","(1) - Nominel kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m.","(1) - Nominel kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","","","","","","","","","","","","","","(2) - Se særskilte tegninger med de elektriske data","(2) - Se særskilte tegninger med de elektriske data","(2) - Se særskilte tegninger med de elektriske data","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["Energieffektivitetsklasse","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Bemærkninger","","","","","","","","","","","","","","","","","","","","(3) - Se separat tegning for driftsområde","(3) - Se separat tegning for driftsområde","(3) - Se separat tegning for driftsområde"]
["","","","","","","","","","","","","","","","","","","","","(4) - Se særskilte tegninger med de elektriske data","(4) - Se særskilte tegninger med de elektriske data","(4) - Se særskilte tegninger med de elektriske data"]