{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L9V1B","FCAG71BVEB / FCAG71BVEB / RZQG100L9V1B"]
["Kølekapacitet","Nom.","","kW","9.50","9.50"]
["Nominel effektivitet","EER","","","3.11","3.75"]
["Rumkøling","Energieffektivitetsklasse","","","A","A"]
["","Kapacitet","Pdesign","kW","9.50","9.50"]
["","SEER","","","5.10","5.10"]
["","Årligt energiforbrug","","kWh/a","652","652"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A","A"]
["","Kapacitet","Pdesign","kW","7.60","11.30"]
["","SCOP/A","","","3.81","3.80"]
["","Årligt energiforbrug","","kWh/a","2,791","4,164"]
["Bemærkninger","","","","(1) - Se separat tegning for driftsområde","(1) - Se separat tegning for driftsområde"]
["","","","","(2) - Se særskilte tegninger med de elektriske data","(2) - Se særskilte tegninger med de elektriske data"]